# 2025 Ram Chassis Cab

## FEATURE AVAILABILITY

S = Standard. O = Optional.  P = Part of package. NA = Not available.
Note: some features and/or applications may be late availability.

### CONFIGURATION

|  |  |  |
| --- | --- | --- |
| 3500 – Body Model | TRADESMAN | BIG HORN |
| Regular Cab — 60-in. CA (143.5-in. wheelbase) | S | S |
| Regular Cab — 84-in. CA (167.5-in. wheelbase) | S | S |
| Crew Cab — 60-in. CA (172.4-in. wheelbase) | O | O |

|  |  |  |
| --- | --- | --- |
| 3500 – Drive System | TRADESMAN | BIG HORN |
| 4x2 | S | NA |
| 4x4 | O | S |

| 4500/5500 – Body Model | TRADESMAN | BIG HORN |
| --- | --- | --- |
| Regular Cab — 60-in. CA (144.5-in. wheelbase) | S | S |
| Regular Cab — 84-in. CA (168.5-in. wheelbase) | S | S |
| Regular Cab — 108-in. CA (192.5-in. wheelbase) | S | S |
| Regular Cab — 120-in. CA (204.5-in. wheelbase) | S | S |
| Crew Cab — 60-in. CA (173.4-in. wheelbase) | O | O |
| Crew Cab — 84-in. CA (197.4-in. wheelbase) | O | O |

|  |  |  |
| --- | --- | --- |
| 4500/5500 – Drive System | TRADESMAN | BIG HORN |
| 4x2 | S | S |
| 4x4 | O | O |

### POWERTRAIN

|  |  |  |
| --- | --- | --- |
| Engine / Transmission | TRADESMAN | BIG HORN |
| 6.4-liter HEMIâ V-8 (3500) with TorqueFlite eight-speed 8HP75 automatic transmission | S | S |
| 6.4-liter HEMI V-8 (3500/4500/5500) with eight-speed ZF TorqueFlite HD automatic transmission | S/P | S/P |
| 6.7-liter Cummins Turbo Diesel I-6 engine (3500/4500/5500) with eight-speedZF TorqueFlite HD automatic transmission | O | O |

### MECHANICAL

| Alternator | TRADESMAN | BIG HORN |
| --- | --- | --- |
| 220-amp | S | S |
| 400-amp (dual 220-amp and 180-amp; requires 6.4-liter; included with On-Board Power System) | O/P | O/P |
| 480-amp (dual 240-amp alternators; requires 6.7-liter; included with On-Board Power System) | O/P | O/P |

|  |  |  |
| --- | --- | --- |
| Axles: 3500 | TRADESMAN | BIG HORN |
| Single rear wheel | S | S |
| Dual rear wheel | O | O |
| Front, 6,000-lb. GAWR (SRW axle) | S | S |
| Rear, 11.50-in. (SRW axle) | S | S |
| Front, 205 mm (DRW axle) | S/O | S/O |
| Rear, 11.50-in. (DRW axle) | S/O | S/O |

|  |  |  |
| --- | --- | --- |
| Axle Ratios: 3500 | TRADESMAN | BIG HORN |
| 4.10 ratio (standard with gas) | S | S |
| 3.42 ratio (packaged with diesel models only) | P | P |
| Rear, anti-spin differential | S | S |

|  |  |  |
| --- | --- | --- |
| Axles: 4500/5500 | TRADESMAN | BIG HORN |
| Dual rear wheel | S | S |
| Front, 10.5-in. | S | S |
| Front, 10.5-in., 7,250-lb. GAWR | O | O |
| Front-axle disconnect (4500/5500 included on all 4x4) | P | P |
| Rear, anti-spin differential | S | S |

|  |  |  |
| --- | --- | --- |
| Axle Ratios: 4500 | TRADESMAN | BIG HORN |
| 4.44 ratio | S | S |

|  |  |  |
| --- | --- | --- |
| Axle Ratios: 5500 | TRADESMAN | BIG HORN |
| 4.44 ratio | S | S |

|  |  |  |
| --- | --- | --- |
| Fuel Tank | TRADESMAN | BIG HORN |
| 52-gallon, rear | S | S |
| 74-gallon dual fuel tanks (52 and 22 gals.) | O | O |
| 22-gallon mid-ship fuel tank | O | O |

|  |  |  |
| --- | --- | --- |
| Power Take Off (PTO) | TRADESMAN | BIG HORN |
| Stationary elevated engine idle up | S | S |
| PTO: right-side / left-side (packaged with PTO) | P | P |
| Split-shaft PTO (packaged with PTO on Diesel) | P | P |
| Hard-wired remote start/stop (packaged with PTO) | P | P |

|  |  |  |
| --- | --- | --- |
| Engine Shut-Off Timer | TRADESMAN | BIG HORN |
| 6.4-liter and 6.7-liter (5 minutes) (dealer programmable from 1 to 60 minutes) | O | O |

### INTERIOR

|  |  |  |
| --- | --- | --- |
| Instrument Cluster Displays | TRADESMAN | BIG HORN |
| Cluster 3.5-in. TFT color display | S | S |
| Cluster 7.0-in. TFT color display | P | P |
| Cluster 12.0-in. TFT color display | NA | P |

|  |  |  |
| --- | --- | --- |
| Telematics | TRADESMAN | BIG HORN |
| Connectivity (standard for US / Canada markets) | S | S |
| Upfitter Interface | TRADESMAN | BIG HORN |
| Vehicle system interface module (VSIM) | S | S |

### UCONNECT MULTIMEDIA

|  |  |  |
| --- | --- | --- |
| Bluetooth | TRADESMAN | BIG HORN |
| Uconnect Voice Command with Bluetooth | S | S |
| Compass / GPS | TRADESMAN | BIG HORN |
| Compass display in the radio | S | S |
| GPS antenna input on radio  | S | S |
| Media | TRADESMAN | BIG HORN |
| Front: media hub — includes two fully functional type A/C USB port pairs and one auxiliary jack (four USB connection points) | S | S |
| Middle: 2.5-amp charge-only single USB port (located in center console or armrest) | S | S |
| Rear: dual remote USB port 2 A/C pairs; one pair fully functional,one pair charge only (packaged with Big Horn Level 3) | NA | P |
| Auxiliary headphone jack for mobile devices | S | S |
| Dual wireless charging pad (packaged with Big Horn Level 3) | NA | P |

|  |  |  |
| --- | --- | --- |
| Power | TRADESMAN | BIG HORN |
| Accessory delay | S | S |
| Auxiliary outlets (one battery and one ignition-fed) | S | S |
| 115-volt auxiliary power outlet w/ 400-watt inverter, instrument panel-mounted  | P | P |
| 115-volt auxiliary power outlet, rear facing (packaged with Big Horn Level 3) | NA | P |
| 2.4kW on-board power system | O | O |

|  |  |  |
| --- | --- | --- |
| Radios | TRADESMAN | BIG HORN |
| Uconnect 8.4 — AM/FM/BT/SiriusXM with 8.4-in. touchscreen display, Apple CarPlay and Android Auto, Uconnect with Bluetooth, SiriusXM Radio | S | S |
| Uconnect 12.0 — AM/FM/BT/SiriusXM/Nav with 12.0-in. touchscreen display, GPS Navigation, Apple CarPlay and Android Auto, Uconnect with Bluetooth, SiriusXM Radio | P | P |
| Radio controls, steering wheel-mounted audio controls | P | P |

### SAFETY AND SECURITY

| Camera | TRADESMAN | BIG HORN |
| --- | --- | --- |
| ParkView rear backup camera | O | O |
| Cargo View Camera requires 12-in. radio, includes LED CHMSL and cargo lamps (packaged with Big Horn Level 2 & 3) | NA | P |
| Auxiliary wired camera (Mopar camera available at dealer) | O | O |
| Digital rearview mirror camera relocation kit | O | O |

| Parking Sensors | TRADESMAN | BIG HORN |
| --- | --- | --- |
| Rear park assist | O | O |
| ParkSense front/rear park assist | O | O/P |

| Safety Features | TRADESMAN | BIG HORN |
| --- | --- | --- |
| Security alarm | P | P |
| Backup alarm (audible alarm when vehicle is in reverse) | O | O |
| Lane Departure Warning, (Lane Keep Assist) | P | P |
| Adaptive steering | P | P |
| Adaptive Cruise Control with Stop | S | S |
| Ready Alert Braking | S | S |
| Full-speed Forward Collision Warning-Plus | S | S |
| Pedestrian Automatic Emergency Braking | P | P |
| Max speed settings (65 mph, 70 mph, 77 mph) | O | O |
| Auto high-beam headlamp control | P | P |
| Rain-sensing wipers | P | P |
| Drowsy Driver Detection | P | P |
| Traffic Sign Recognition | P | P |
| Auxiliary reverse lamps (packaged with Big Horn Level 3) | NA | P |

### EQUIPMENT PACKAGES

| EQUIPMENT PACKAGES | TRADESMAN | BIG HORN |
| --- | --- | --- |
| **Ambulance Prep Group**Remote rear heat/AC (provides ability to run auxiliary-mounted heater and A/C independently of instrument panel controls)A/C line tap and engine coolant access for upfitterFoam roof blocks (included with Regular Cab only) | O | O |
| **Chrome Appearance Group**Chrome front bumper (3500/4500/5500) Chrome grille (3500/4500/5500)Chrome insertsPolished aluminum wheels on 3500Bright wheel cover (4500/5500) | O | NA |
| **Cold Weather Group (Diesel option)**Engine block heater cordWinter front grille cover | O | O |
| **Tradesman Level 1 Equipment Group**Overhead console (Regular Cab)Power windows (Regular Cab)Power door locks (Regular Cab) (speed-sensitive actuation)Black trailer tow mirrors (Regular Cab)Door trim: (Regular Cab) (wrapped bolster/armrest, 360 door handles, join seam, Iron Gray-painted surround and accent)Remote keyless entry (Regular Cab)Rear window defroster | O | NA |
| **Tradesman Level 2 Equipment Group**Tradesman Level 1 content115V power outlet12.0-inch radioDual zone ACPower-sliding rear window (Crew Cab)Remote startTinted acoustic windshieldDigital rearview mirrorPower 2-way driver lumbarTrailer brake controlBlack wheel flares (3500) | O | NA |
| **Big Horn Level 1 Equipment Group**Power-sliding rear window (Crew Cab)Rear window defroster115V power outletDual glove boxesFoam bottle door trim panel insertCluster 7.0-in. TFT color displayGlove box lampRear dome lampLeather-wrapped steering wheelRemote startDigital rearview mirror12.0-in. radioDual zone ACNine Alpine speakers w/ subwoofer (Crew Cab)Premium speakers (Regular Cab)Black wheel flares (3500) | NA | O |
| **Big Horn Level 2 Equipment Group**Big Horn Level 1 contentCHMSL lamp w/ cameraDigital cargo cameraUniversal garage door openerPower 2-way driver lumbarPolished aluminum wheels (set of 4) | NA | O |
| **Big Horn Level 3 Equipment Group Laramie Package (Crew Cab 4x4 only)**Big Horn Level 2 contentParkSense front/rear park assistPainted body-color front bumper, wheel flares & door handlesUnique grilleAuto high beam headlamp controlHigh-level signature LED headlampsDaytime running lampsI/P bezels — painted w/ premium filmOverhead console — premiumRear media hub w/ 2 USB A/C (charge only)Remote proximity passive keyless entryWrapped & stitched bolster & plated speaker trim ringCluster 12.0-in. TFT color displayFront & rear door handle w/ LED lightsMap courtesy LED lampsSwitchable LED dome lampsFootwell LED lampsDual wireless charging padUltra-premium 17 amplified speakers w/ subwooferRain-sensing wipersLT225/70R19.5 off-road tiresFront high-back bucket seats8-way power driver and passenger seatsHeated and ventilated driver and passenger seatHeated steering wheel4-way front headrests, driver and passengerFull length upgraded floor console w/ 2 front & 2 rear cupholders60/40-fold up rear seat w/ center fold down arm rest2-way adjustable rear head restHeated rear seatsFold-flat load floor | NA | O |
| **Safety Group**Security alarmLane Keep AssistAdaptive steeringRain-sensing wipersTraffic Sign RecognitionDrowsy Driver DetectionCluster 7.0-in. TFT color displayDigital rearview mirrorAuto high-beam headlamp control | O | O |
| **Max Tow Package (Requires Diesel, 5500 only)**Max tow electronic shift-on-the-fly transfer caseTrailer brake controller | O | O |
| **Max Payload Package (6.4-liter 5500 only)**19,000-lb. GVWR or 19,500-lb. GVWR | O | O |
| **Rear Interior Trim Delete Group (Regular Cab only, Fleet only)**Delete front center seatDelete rear floor storage trayDelete cab back trim panel | O | O |
| **15,000-lb. GVWR Package (4500 only)**Includes 15,000-lb. Gross Vehicle Weight Rating 4x2, 4x4 | O | O |
| **16,000 GVWR Package (4500 only)**Includes 16,000-lb. Gross Vehicle Weight Rating 4x2, 4x4 | O | O |

###