# 2025 Ram Chassis Cab

## FEATURE AVAILABILITY

S = Standard. O = Optional.  P = Part of package. NA = Not available.   
Note: some features and/or applications may be late availability.

### CONFIGURATION

|  |  |  |
| --- | --- | --- |
| 3500 – Body Model | TRADESMAN | BIG HORN |
| Regular Cab — 60-in. CA (143.5-in. wheelbase) | S | S |
| Regular Cab — 84-in. CA (167.5-in. wheelbase) | S | S |
| Crew Cab — 60-in. CA (172.4-in. wheelbase) | O | O |

|  |  |  |
| --- | --- | --- |
| 3500 – Drive System | TRADESMAN | BIG HORN |
| 4x2 | S | NA |
| 4x4 | O | S |

| 4500/5500 – Body Model | TRADESMAN | BIG HORN |
| --- | --- | --- |
| Regular Cab — 60-in. CA (144.5-in. wheelbase) | S | S |
| Regular Cab — 84-in. CA (168.5-in. wheelbase) | S | S |
| Regular Cab — 108-in. CA (192.5-in. wheelbase) | S | S |
| Regular Cab — 120-in. CA (204.5-in. wheelbase) | S | S |
| Crew Cab — 60-in. CA (173.4-in. wheelbase) | O | O |
| Crew Cab — 84-in. CA (197.4-in. wheelbase) | O | O |

|  |  |  |
| --- | --- | --- |
| 4500/5500 – Drive System | TRADESMAN | BIG HORN |
| 4x2 | S | S |
| 4x4 | O | O |

### POWERTRAIN

|  |  |  |
| --- | --- | --- |
| Engine / Transmission | TRADESMAN | BIG HORN |
| 6.4-liter HEMIâ V-8 (3500) with TorqueFlite eight-speed 8HP75 automatic transmission | S | S |
| 6.4-liter HEMI V-8 (3500/4500/5500) with eight-speed ZF TorqueFlite HD automatic transmission | S/P | S/P |
| 6.7-liter Cummins Turbo Diesel I-6 engine (3500/4500/5500) with eight-speed ZF TorqueFlite HD automatic transmission | O | O |

### MECHANICAL

| Alternator | TRADESMAN | BIG HORN |
| --- | --- | --- |
| 220-amp | S | S |
| 400-amp (dual 220-amp and 180-amp; requires 6.4-liter; included with On-Board Power System) | O/P | O/P |
| 480-amp (dual 240-amp alternators; requires 6.7-liter; included with On-Board Power System) | O/P | O/P |

|  |  |  |
| --- | --- | --- |
| Axles: 3500 | TRADESMAN | BIG HORN |
| Single rear wheel | S | S |
| Dual rear wheel | O | O |
| Front, 6,000-lb. GAWR (SRW axle) | S | S |
| Rear, 11.50-in. (SRW axle) | S | S |
| Front, 205 mm (DRW axle) | S/O | S/O |
| Rear, 11.50-in. (DRW axle) | S/O | S/O |

|  |  |  |
| --- | --- | --- |
| Axle Ratios: 3500 | TRADESMAN | BIG HORN |
| 4.10 ratio (standard with gas) | S | S |
| 3.42 ratio (packaged with diesel models only) | P | P |
| Rear, anti-spin differential | S | S |

|  |  |  |
| --- | --- | --- |
| Axles: 4500/5500 | TRADESMAN | BIG HORN |
| Dual rear wheel | S | S |
| Front, 10.5-in. | S | S |
| Front, 10.5-in., 7,250-lb. GAWR | O | O |
| Front-axle disconnect (4500/5500 included on all 4x4) | P | P |
| Rear, anti-spin differential | S | S |

|  |  |  |
| --- | --- | --- |
| Axle Ratios: 4500 | TRADESMAN | BIG HORN |
| 4.44 ratio | S | S |

|  |  |  |
| --- | --- | --- |
| Axle Ratios: 5500 | TRADESMAN | BIG HORN |
| 4.44 ratio | S | S |

|  |  |  |
| --- | --- | --- |
| Fuel Tank | TRADESMAN | BIG HORN |
| 52-gallon, rear | S | S |
| 74-gallon dual fuel tanks (52 and 22 gals.) | O | O |
| 22-gallon mid-ship fuel tank | O | O |

|  |  |  |
| --- | --- | --- |
| Power Take Off (PTO) | TRADESMAN | BIG HORN |
| Stationary elevated engine idle up | S | S |
| PTO: right-side / left-side (packaged with PTO) | P | P |
| Split-shaft PTO (packaged with PTO on Diesel) | P | P |
| Hard-wired remote start/stop (packaged with PTO) | P | P |

|  |  |  |
| --- | --- | --- |
| Engine Shut-Off Timer | TRADESMAN | BIG HORN |
| 6.4-liter and 6.7-liter (5 minutes) (dealer programmable from 1 to 60 minutes) | O | O |

### INTERIOR

|  |  |  |
| --- | --- | --- |
| Instrument Cluster Displays | TRADESMAN | BIG HORN |
| Cluster 3.5-in. TFT color display | S | S |
| Cluster 7.0-in. TFT color display | P | P |
| Cluster 12.0-in. TFT color display | NA | P |

|  |  |  |
| --- | --- | --- |
| Telematics | TRADESMAN | BIG HORN |
| Connectivity (standard for US / Canada markets) | S | S |
| Upfitter Interface | TRADESMAN | BIG HORN |
| Vehicle system interface module (VSIM) | S | S |

### UCONNECT MULTIMEDIA

|  |  |  |
| --- | --- | --- |
| Bluetooth | TRADESMAN | BIG HORN |
| Uconnect Voice Command with Bluetooth | S | S |
| Compass / GPS | TRADESMAN | BIG HORN |
| Compass display in the radio | S | S |
| GPS antenna input on radio | S | S |
| Media | TRADESMAN | BIG HORN |
| Front: media hub — includes two fully functional type A/C USB port pairs  and one auxiliary jack (four USB connection points) | S | S |
| Middle: 2.5-amp charge-only single USB port (located in center console  or armrest) | S | S |
| Rear: dual remote USB port 2 A/C pairs; one pair fully functional, one pair charge only (packaged with Big Horn Level 3) | NA | P |
| Auxiliary headphone jack for mobile devices | S | S |
| Dual wireless charging pad (packaged with Big Horn Level 3) | NA | P |

|  |  |  |
| --- | --- | --- |
| Power | TRADESMAN | BIG HORN |
| Accessory delay | S | S |
| Auxiliary outlets (one battery and one ignition-fed) | S | S |
| 115-volt auxiliary power outlet w/ 400-watt inverter, instrument panel-mounted | P | P |
| 115-volt auxiliary power outlet, rear facing (packaged with Big Horn Level 3) | NA | P |
| 2.4kW on-board power system | O | O |

|  |  |  |
| --- | --- | --- |
| Radios | TRADESMAN | BIG HORN |
| Uconnect 8.4 — AM/FM/BT/SiriusXM with 8.4-in. touchscreen display, Apple CarPlay  and Android Auto, Uconnect with Bluetooth, SiriusXM Radio | S | S |
| Uconnect 12.0 — AM/FM/BT/SiriusXM/Nav with 12.0-in. touchscreen display, GPS Navigation,  Apple CarPlay and Android Auto, Uconnect with Bluetooth, SiriusXM Radio | P | P |
| Radio controls, steering wheel-mounted audio controls | P | P |

### SAFETY AND SECURITY

| Camera | TRADESMAN | BIG HORN |
| --- | --- | --- |
| ParkView rear backup camera | O | O |
| Cargo View Camera requires 12-in. radio, includes LED CHMSL  and cargo lamps (packaged with Big Horn Level 2 & 3) | NA | P |
| Auxiliary wired camera (Mopar camera available at dealer) | O | O |
| Digital rearview mirror camera relocation kit | O | O |

| Parking Sensors | TRADESMAN | BIG HORN |
| --- | --- | --- |
| Rear park assist | O | O |
| ParkSense front/rear park assist | O | O/P |

| Safety Features | TRADESMAN | BIG HORN |
| --- | --- | --- |
| Security alarm | P | P |
| Backup alarm (audible alarm when vehicle is in reverse) | O | O |
| Lane Departure Warning, (Lane Keep Assist) | P | P |
| Adaptive steering | P | P |
| Adaptive Cruise Control with Stop | S | S |
| Ready Alert Braking | S | S |
| Full-speed Forward Collision Warning-Plus | S | S |
| Pedestrian Automatic Emergency Braking | P | P |
| Max speed settings (65 mph, 70 mph, 77 mph) | O | O |
| Auto high-beam headlamp control | P | P |
| Rain-sensing wipers | P | P |
| Drowsy Driver Detection | P | P |
| Traffic Sign Recognition | P | P |
| Auxiliary reverse lamps (packaged with Big Horn Level 3) | NA | P |

### EQUIPMENT PACKAGES

| EQUIPMENT PACKAGES | TRADESMAN | BIG HORN | |
| --- | --- | --- | --- |
| **Ambulance Prep Group**  Remote rear heat/AC (provides ability to run auxiliary-mounted heater  and A/C independently of instrument panel controls)  A/C line tap and engine coolant access for upfitter  Foam roof blocks (included with Regular Cab only) | O | O | |
| **Chrome Appearance Group**  Chrome front bumper (3500/4500/5500)  Chrome grille (3500/4500/5500)  Chrome inserts  Polished aluminum wheels on 3500  Bright wheel cover (4500/5500) | O | NA | |
| **Cold Weather Group (Diesel option)**  Engine block heater cord  Winter front grille cover | O | O | |
| **Tradesman Level 1 Equipment Group**  Overhead console (Regular Cab)  Power windows (Regular Cab)  Power door locks (Regular Cab) (speed-sensitive actuation)  Black trailer tow mirrors (Regular Cab)  Door trim: (Regular Cab) (wrapped bolster/armrest, 360 door handles,  join seam, Iron Gray-painted surround and accent)  Remote keyless entry (Regular Cab)  Rear window defroster | O | NA | |
| **Tradesman Level 2 Equipment Group**  Tradesman Level 1 content  115V power outlet  12.0-inch radio  Dual zone AC  Power-sliding rear window (Crew Cab)  Remote start  Tinted acoustic windshield  Digital rearview mirror  Power 2-way driver lumbar  Trailer brake control  Black wheel flares (3500) | O | NA | |
| **Big Horn Level 1 Equipment Group**  Power-sliding rear window (Crew Cab)  Rear window defroster  115V power outlet  Dual glove boxes  Foam bottle door trim panel insert  Cluster 7.0-in. TFT color display  Glove box lamp  Rear dome lamp  Leather-wrapped steering wheel  Remote start  Digital rearview mirror  12.0-in. radio  Dual zone AC  Nine Alpine speakers w/ subwoofer (Crew Cab)  Premium speakers (Regular Cab)  Black wheel flares (3500) | NA | O | |
| **Big Horn Level 2 Equipment Group**  Big Horn Level 1 content  CHMSL lamp w/ camera  Digital cargo camera  Universal garage door opener  Power 2-way driver lumbar  Polished aluminum wheels (set of 4) | | NA | | O |
| **Big Horn Level 3 Equipment Group  Laramie Package (Crew Cab 4x4 only)**  Big Horn Level 2 content  ParkSense front/rear park assist  Painted body-color front bumper, wheel flares & door handles  Unique grille  Auto high beam headlamp control  High-level signature LED headlamps  Daytime running lamps  I/P bezels — painted w/ premium film  Overhead console — premium  Rear media hub w/ 2 USB A/C (charge only)  Remote proximity passive keyless entry  Wrapped & stitched bolster & plated speaker trim ring  Cluster 12.0-in. TFT color display  Front & rear door handle w/ LED lights  Map courtesy LED lamps  Switchable LED dome lamps  Footwell LED lamps  Dual wireless charging pad  Ultra-premium 17 amplified speakers w/ subwoofer  Rain-sensing wipers  LT225/70R19.5 off-road tires  Front high-back bucket seats  8-way power driver and passenger seats  Heated and ventilated driver and passenger seat  Heated steering wheel  4-way front headrests, driver and passenger  Full length upgraded floor console w/ 2 front & 2 rear cupholders  60/40-fold up rear seat w/ center fold down arm rest  2-way adjustable rear head rest  Heated rear seats  Fold-flat load floor | NA | | O |
| **Safety Group**  Security alarm  Lane Keep Assist  Adaptive steering  Rain-sensing wipers  Traffic Sign Recognition  Drowsy Driver Detection  Cluster 7.0-in. TFT color display  Digital rearview mirror  Auto high-beam headlamp control | O | | O |
| **Max Tow Package (Requires Diesel, 5500 only)**  Max tow electronic shift-on-the-fly transfer case  Trailer brake controller | O | | O |
| **Max Payload Package (6.4-liter 5500 only)**  19,000-lb. GVWR or 19,500-lb. GVWR | O | | O |
| **Rear Interior Trim Delete Group (Regular Cab only, Fleet only)**  Delete front center seat  Delete rear floor storage tray  Delete cab back trim panel | O | | O |
| **15,000-lb. GVWR Package (4500 only)**  Includes 15,000-lb. Gross Vehicle Weight Rating 4x2, 4x4 | O | O | |
| **16,000 GVWR Package (4500 only)**  Includes 16,000-lb. Gross Vehicle Weight Rating 4x2, 4x4 | O | O | |

###